{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":53,"n_cols":4,"rows_kept":53,"merged":[[0,0,0,3],[52,0,52,3]],"flags":["formulas_cached_only"]}
["2025年防雷装置接地检测范围"]
["项目","测点数","项目","测点数"]
["氢站避雷针",1,"生产综合楼：避雷带",8]
["氢站罐区: 管道、法兰盘",15,"接地极",6]
["储气罐",4,"消防管道",4]
["氢储气罐1号—4号",8,"综合水泵房旁：4个水罐、管道",12]
["防静电装置",4,"综合水泵房后：红罐、法兰盘",6]
["桥架",10,"净水站栏杆及桥架",8]
["汇流排充氢门及排空管",10,"化水区域避2根雷针",4]
["干燥器、电解槽等设备",10,"废水区：酸罐",6]
["低压抽出式开关柜、整流柜",2,"碱罐",6]
["制氢站电子间控制柜",2,"次氯酸钠罐",6]
["螺旋板式换热器：管道、罐、法兰盘",8,"爬梯、栏杆、钢架棚",10]
["纯水箱、碱液箱",6,"4个罐",16]
["防爆灯1、2灯杆",4,"法兰盘、管道",10]
["检修试验楼：避雷带",8,"输煤-化水综合管架",20]
["接地极",6,"氢站-主厂房-行政楼后综合管架",6]
["冷却塔1：接地极、爬梯、管道",8,"生活污水处理成套设备：爬梯、平台",4]
["冷却塔2：接地极、爬梯、管道",8,"生活污水处理成套设备：管道",4]
["贮燃油罐1号、2号避雷针",4,"灰库顶设备、管道及爬梯",10]
["贮燃油泵房区：8盏防爆灯杆",8,"汽机房A列房顶避雷针",8]
["油罐1、2",6,"汽机房顶氢、油箱排空管",8]
["油罐区爬梯、法兰盘、管道",24,"汽机房线架",6]
["打孔滤油器1—5",20,"输煤#9、#5、#4、#3栈桥",8]
["防爆防水接线盒1—5",25,"#1、#2锅炉及电除尘构架",8]
["供油泵1号、2号、3号",6,"渣仓A、B工作平台及楼梯",8]
["卸油泵及接头",7,"电除尘主体构架",4]
["管道、法兰盘",6,"新石膏库避雷带及扩建端楼梯",4]
["槽架",8,"#1、#2脱硫一、二号吸收塔",10]
["管道支撑架",6,"新老斗提机库顶设备、栏杆及爬梯",6]
["煤仓间、桥架、桥架与支撑柱",20,"推土机库",2]
["碎煤机室、碎煤机、管道、避雷带、爬梯",10,"乙炔库房避雷针",1]
["烟囱接地体及扁铁",8,"氧气乙炔库",2]
["化学楼后：1#、2#除盐水箱、爬梯、管道",16,"煤场灯塔",4]
["混床用压缩空气储罐              ",4,"干煤棚",4]
["酸罐1、2",12,"斗轮机及轨道",4]
["碱罐1、2",12,"生活区#2、#3、#4、#6、#9、#10楼、食堂、羽毛球馆",20]
["氨区： 1#避雷针",2,"生活区箱变及分支箱",6]
["1、2、3#液氨储罐",12,"启动锅炉房烟囱",2]
["1、2#金属棚",4,"锅炉房爬梯（扩建端侧）",2]
["1、2#气氨缓冲罐",8,"汽机房立柱接地引下线",10]
["气氨稀释槽",4,"汽机房支撑架",8]
["爬梯",4,"汽机房法兰盘、管道、栏杆",15]
["栏杆",4,"汽机房EH、润滑油箱",8]
["1、2#液氨蒸发器",4,"江边取水升压变避雷针、翻车机控制楼、翻车机顶棚以及本体",10]
["消防炮",8,"江边取水泵房区域：泵房、避雷针、配电室、生活间、取水降压变、取水泵电机",20]
["监控值班室及避雷带",4]
["静电触摸柱",4]
["尿素制氨区A/B溶液储罐、疏水箱、水解橇顶棚、静电释放装置、控制室/尿素堆料间避雷带以及脱硫新增事故浆液箱、楼梯等",20]
["水解橇基座、产品气管道构架",10]
[]
[]
["注：具体检测点以现场实际为准，与本清单或许存在一定出入。"]